|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S/s** | **Name of goods** | **Standart of goods** | **Measurement** | **Quantity** | **PRICE** |
| **LOT-1** | | | | |  |
| 1 | Armored dip cable with rounded (KPBK-90 type)  Dimensions - 3x25 mm²  Tension - up to 3300V  Working temperature - up to 90 ° C | GOST P51777-2001  TU 16-505.129-82 | meter | 2 000 |  |
| 2 | Armored dip cable with rounded (KPBK-90 type)  Dimensions - 3x35 mm²  Tension - up to 3300V  Working temperature - up to 90 ° C | GOST P51777-2001  TU 16-505.129-82 | meter | 1 400 |  |
| 3 | Armored dip cable with rounded (KPBP-90 type)  Dimensions - 3x10 mm²  Tension - up to 3300V  Working temperature - up to 90 ° C | GOST P51777-2001  TU 16-505.129-82 | meter | 10 500 |  |
| 4 | Armored dip cable with rounded (KPBK-90 type)  Dimensions - 3x10 mm²  Tension - up to 3300V  Working temperature - up to 90 ° C | GOST P51777-2001  TU 16-505.129-82 | meter | 40 000 |  |
| 5 | Armored dip cable with rounded (KPBK-90 type)  Dimensions - 3x16 mm²  Tension - up to 3300V  Working temperature - up to 90 ° C | GOST P51777-2001  TU 16-505.129-82 | meter | 16 000 |  |